- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# pll_drv.h

Go to the documentation of this file.

    00001 /*This file has been prepared for Doxygen automatic documentation generation.*/
    00013
    00014 /* Copyright (c) 2007, Atmel Corporation All rights reserved.
    00015  *
    00016  * Redistribution and use in source and binary forms, with or without
    00017  * modification, are permitted provided that the following conditions are met:
    00018  *
    00019  * 1. Redistributions of source code must retain the above copyright notice,
    00020  * this list of conditions and the following disclaimer.
    00021  *
    00022  * 2. Redistributions in binary form must reproduce the above copyright notice,
    00023  * this list of conditions and the following disclaimer in the documentation
    00024  * and/or other materials provided with the distribution.
    00025  *
    00026  * 3. The name of ATMEL may not be used to endorse or promote products derived
    00027  * from this software without specific prior written permission.
    00028  *
    00029  * THIS SOFTWARE IS PROVIDED BY ATMEL ``AS IS'' AND ANY EXPRESS OR IMPLIED
    00030  * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
    00031  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT ARE EXPRESSLY AND
    00032  * SPECIFICALLY DISCLAIMED. IN NO EVENT SHALL ATMEL BE LIABLE FOR ANY DIRECT,
    00033  * INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
    00034  * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
    00035  * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
    00036  * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
    00037  * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
    00038  * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
    00039  */
    00040
    00041 #ifndef PLL_DRV_H
    00042 #define PLL_DRV_H
    00043
    00044 //_____ I N C L U D E S ____________________________________________________
    00045
    00049 //_____ M A C R O S ________________________________________________________
    00050
    00054 #define PLLx06          ( (0<<PLLP2) | (1<<PLLP1) | (1<<PLLP0) )
    00055
    00056 #ifdef __ICCAVR__
    00057    #if (defined(__AT90USB1287__) || defined(__AT90USB1286__))
    00058       #define PLLx03          ( (1<<PLLP2) | (0<<PLLP1) | (1<<PLLP0) )
    00059    #elif (defined(__AT90USB647__) || defined(__AT90USB646__) || defined(__ATmega32U6__))
    00060       #define PLLx03          ( (1<<PLLP2) | (1<<PLLP1) | (0<<PLLP0) )
    00061    #else
    00062       #error TARGET should be defined
    00063    #endif
    00064 #elif defined __GNUC__
    00065    #if (defined(__AVR_AT90USB1287__) || defined(__AVR_AT90USB1286__))
    00066       #define PLLx03          ( (1<<PLLP2) | (0<<PLLP1) | (1<<PLLP0) )
    00067    #elif (defined(__AVR_AT90USB647__) || defined(__AVR_AT90USB646__) || defined(__AVR_ATmega32U6__))
    00068       #define PLLx03          ( (1<<PLLP2) | (1<<PLLP1) | (0<<PLLP0) )
    00069    #endif
    00070 #else // Other compiler
    00071    #error Compiler unknow
    00072 #endif
    00073
    00074
    00077 #define Start_pll(clockfactor)   (PLLCSR = ( clockfactor  | (1<<PLLE)  ))
    00079 #define Is_pll_ready()           (PLLCSR & (1<<PLOCK) )
    00081 #define Wait_pll_ready()         while (!(PLLCSR & (1<<PLOCK)))
    00083 #define Stop_pll()               (PLLCSR  &= (~(1<<PLLE)),PLLCSR=0 )
    00084 #ifdef CUSTOM_PLL_START_AUTO
    00085    #define    Pll_start_auto()   CUSTOM_PLL_START_AUTO
    00086 #else
    00087
    00088       // Start the PLL in autofactor mode
    00089       // regarding FOSC define
    00090 #if   (FOSC==8000)
    00091    #define Pll_start_auto()   Start_pll(PLLx06)
    00092 #elif (FOSC==16000)
    00093    #define Pll_start_auto()   Start_pll(PLLx03)
    00094 #else
    00095    #error   "FOSC should be defined with 8000KHz or 16000KHz in config.h"
    00096 #endif
    00097 #endif
    00098
    00100
    00102 #endif  // PLL_DRV_H
    00103
    00104