- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# fs_com.h File Reference

FAT 12/16/32 Services. More...

`#include "conf_explorer.h"`

Include dependency graph for fs_com.h:

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | Fs_index
## Defines
#define | _GLOBEXT_ extern
| Used to have a clear code with only one segment to define a variable in project.
Modes of file name control functions
#define | FS_NAME_GET TRUE
#define | FS_NAME_CHECK FALSE
Modes of disk serial number function
#define | FS_SN_READ TRUE
#define | FS_SN_WRITE FALSE
Modes of disk label function
#define | FS_LABEL_READ TRUE
#define | FS_LABEL_WRITE FALSE
Status returned by paste file function
#define | COPY_BUSY 0x00
#define | COPY_FAIL 0x01
#define | COPY_FINISH 0x02
Date field managed by date control functions
#define | FS_DATE_CREATION TRUE
#define | FS_DATE_LAST_WRITE FALSE
File entry types used by many functions
#define | FS_FILE TRUE
#define | FS_DIR FALSE
Directory identifier, which corresponding at the first cluster of directory cluster list
#define | FS_ID_DIR_EMPTY 0xFFFFFFFF
#define | FS_ID_DIR_ROOT 0
File entry attributes
#define | FS_ATTR_FILE ((Byte)0x00)
#define | FS_ATTR_READ_ONLY ((Byte)0x01)
#define | FS_ATTR_HIDDEN ((Byte)0x02)
#define | FS_ATTR_SYSTEM ((Byte)0x04)
#define | FS_ATTR_VOLUME_ID ((Byte)0x08)
#define | FS_ATTR_DIRECTORY ((Byte)0x10)
#define | FS_ATTR_ARCHIVE ((Byte)0x20)
#define | FS_ATTR_LFN_ENTRY ((Byte)0x0F)
#define | Fat_is_not_a_file ((FS_ATTR_DIRECTORY & fs_g_nav_entry.u8_attr) || (FS_ATTR_VOLUME_ID & fs_g_nav_entry.u8_attr))
File open modes
#define | FOPEN_READ_ACCESS 0x01
#define | FOPEN_WRITE_ACCESS 0x02
#define | FOPEN_CLEAR_SIZE 0x04
#define | FOPEN_CLEAR_PTR 0x08
#define | FOPEN_MODE_R (FOPEN_READ_ACCESS|FOPEN_CLEAR_PTR)
| R access, flux pointer = 0, size not modify.
#define | FOPEN_MODE_R_PLUS (FOPEN_READ_ACCESS|FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR)
| R/W access, flux pointer = 0, size not modify.
#define | FOPEN_MODE_W (FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR|FOPEN_CLEAR_SIZE)
| W access, flux pointer = 0, size = 0.
#define | FOPEN_MODE_W_PLUS (FOPEN_READ_ACCESS|FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR|FOPEN_CLEAR_SIZE)
| R/W access, flux pointer = 0, size = 0.
#define | FOPEN_MODE_APPEND (FOPEN_WRITE_ACCESS)
| W access, flux pointer = at the end, size not modify.
Value to signal the end of file after a file_getc() call
#define | FS_EOF 0xFFFF
Options of format function
#define | FS_FORMAT_DEFAULT 0x01
| The format routine chooses the better FAT for the device.
#define | FS_FORMAT_FAT 0x02
| Force FAT12 or FAT16 format.
#define | FS_FORMAT_FAT32 0x03
| Force FAT32 format.
#define | FS_FORMAT_NOMBR_FLAG 0x80
| MBR is mandatory for USB device on MacOS, and no MBR is mandatory for CD-ROM USB device on Windows.
#define | FS_FORMAT_DEFAULT_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_DEFAULT)
#define | FS_FORMAT_FAT_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_FAT)
#define | FS_FORMAT_FAT32_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_FAT32)
File System errors list
#define | FS_ERR_HW (FAIL+0)
| Hardware driver error.
#define | FS_ERR_NO_FORMAT (FAIL+1)
| The selected drive isn't formated.
#define | FS_ERR_NO_PART (FAIL+2)
| The selected partition doesn't existed.
#define | FS_ERR_NO_SUPPORT_PART (FAIL+3)
| The selected partition isn't supported.
#define | FS_ERR_TOO_FILE_OPEN (FAIL+4)
| The navigation have already opened a file.
#define | FS_ERR_END_OF_DRIVE (FAIL+5)
| There are not other driver.
#define | FS_ERR_BAD_POS (FAIL+6)
| The position is over the file.
#define | FS_ERR_FS (FAIL+7)
| File system error.
#define | FS_ERR_NO_FIND (FAIL+8)
| File no found.
#define | FS_ERR_ENTRY_EMPTY (FAIL+9)
| File entry empty.
#define | FS_ERR_ENTRY_BAD (FAIL+10)
| File entry bad.
#define | FS_ERR_ENTRY_BADTYPE (FAIL+11)
| File entry type don't corresponding.
#define | FS_ERR_NO_DIR (FAIL+12)
| The selected file isn't a directory.
#define | FS_ERR_NO_MOUNT (FAIL+13)
| The partition isn't mounted.
#define | FS_ERR_NO_FILE_SEL (FAIL+14)
| There are no selected file.
#define | FS_NO_LAST_LFN_ENTRY (FAIL+15)
| The file entry isn't the last long file entry.
#define | FS_ERR_ID_FILE (FAIL+17)
| The file identifier is bad.
#define | FS_ERR_NO_FILE (FAIL+18)
| The selected file entry isn't a file.
#define | FS_LUN_WP (FAIL+19)
| Drive is in read only mode.
#define | FS_ERR_READ_ONLY (FAIL+20)
| File is on read access only.
#define | FS_ERR_NAME_INCORRECT (FAIL+21)
| The name don't corresponding at the filter name.
#define | FS_ERR_FILE_NO_OPEN (FAIL+22)
| No file is opened.
#define | FS_ERR_HW_NO_PRESENT (FAIL+23)
| Device is not present.
#define | FS_ERR_IS_ROOT (FAIL+24)
| There aren't parent because the current directory is a root directory.
#define | FS_ERR_OUT_LIST (FAIL+25)
| The position is outside the cluster list.
#define | FS_ERR_NO_FREE_SPACE (FAIL+26)
| No free cluster found in FAT.
#define | FS_ERR_INCORRECT_NAME (FAIL+27)
| Incorrect name, this one cannot contain any of the following characters \/:*?"<>|.
#define | FS_ERR_DIR_NOT_EMPTY (FAIL+28)
| This function erases only file and empty directory.
#define | FS_ERR_WRITE_ONLY (FAIL+29)
| File is on write access only.
#define | FS_ERR_MODE_NOAVIALABLE (FAIL+30)
| This open mode isn't available.
#define | FS_ERR_EOF (FAIL+31)
| End of file.
#define | FS_ERR_BAD_SIZE_FAT (FAIL+32)
| The disk size is not supported by selected FAT format.
#define | FS_ERR_COMMAND (FAIL+33)
| This command is not supported.
#define | FS_ERR_BUFFER_FULL (FAIL+34)
| Buffer is too small.
#define | FS_ERR_COPY_DIR (FAIL+35)
| Directory copy is not supported.
#define | FS_ERR_COPY_RUNNING (FAIL+36)
| A copy action is always running.
#define | FS_ERR_COPY_IMPOSSIBLE (FAIL+37)
| The copy is impossible.
#define | FS_ERR_BAD_NAV (FAIL+38)
| The navigator identifier doesn't existed.
#define | FS_ERR_FILE_OPEN (FAIL+39)
| The file is already opened.
#define | FS_ERR_FILE_OPEN_WR (FAIL+40)
| The file is already opened in write mode.
#define | FS_ERR_FILE_EXIST (FAIL+41)
| The file is already existed.
#define | FS_ERR_NAME_TOO_LARGE (FAIL+42)
| The file name is too large (>260 characters).
#define | FS_ERR_PL_NOT_OPEN (FAIL+50)
| The play list isn't opened.
#define | FS_ERR_PL_ALREADY_OPEN (FAIL+51)
| The play list is already opened.
#define | FS_ERR_PL_LST_END (FAIL+52)
| You are at the end of play list.
#define | FS_ERR_PL_LST_BEG (FAIL+53)
| You are at the beginning of play list.
#define | FS_ERR_PL_OUT_LST (FAIL+54)
| You are outside of the play list.
#define | FS_ERR_PL_READ_ONLY (FAIL+55)
| Impossible to modify the play list.
Compilation feature levels
#define | FSFEATURE_READ 0x00
| All read functions.
#define | FSFEATURE_WRITE 0x02
| nav_file_copy(), nav_file_paste(), nav_file_del(), file_create(), file_open(MODE_WRITE), file_write(), file_putc()
#define | FSFEATURE_WRITE_COMPLET 0x06
| FSFEATURE_WRITE + nav_drive_format(), nav_dir_make(), nav_file_rename(), nav_file_dateset(), nav_file_attributset().
#define | FSFEATURE_ALL 0xFF
| All file system module.
## Typedefs
String types depend of ASCII and UNICODE options
typedef U16 | UNICODE
typedef char _MEM_TYPE_SLOW_ * | FS_STRING
typedef UNICODE _MEM_TYPE_SLOW_ * | FS_STR_UNICODE
Status type for the file system
typedef U8 | Fs_status
## Variables
Global status of file system module (used to return error number)
_MEM_TYPE_SLOW_ Fs_status | fs_g_status

## Detailed Description

FAT 12/16/32 Services.

This file provides a set of definitions for FAT module interface.

Author:
  Atmel Corporation: http://www.atmel.com
  Support and FAQ: http://support.atmel.no/

Definition in file fs_com.h.

## Define Documentation

#define _GLOBEXT_ extern

Used to have a clear code with only one segment to define a variable in project.

Definition at line 50 of file fs_com.h.

#define FS_NAME_GET TRUE

Definition at line 81 of file fs_com.h.

Referenced by copy_dir(), fat_entry_longname(), fat_entry_shortname(), nav_dir_name(), nav_file_getname(), nav_file_name(), nav_getcwd(), ushell_cmd_copy(), ushell_cmd_ls(), and ushell_cmd_sync().

#define FS_NAME_CHECK FALSE

Definition at line 82 of file fs_com.h.

Referenced by nav_filelist_findname().

#define FS_SN_READ TRUE

Definition at line 87 of file fs_com.h.

#define FS_SN_WRITE FALSE

Definition at line 88 of file fs_com.h.

#define FS_LABEL_READ TRUE

Definition at line 93 of file fs_com.h.

Referenced by nav_partition_label().

#define FS_LABEL_WRITE FALSE

Definition at line 94 of file fs_com.h.

Referenced by nav_partition_label().

#define COPY_BUSY 0x00

Definition at line 99 of file fs_com.h.

Referenced by copy_dir(), ushell_cmd_copy(), and ushell_cmd_sync().

#define COPY_FAIL 0x01

Definition at line 100 of file fs_com.h.

Referenced by ushell_cmd_copy().

#define COPY_FINISH 0x02

Definition at line 101 of file fs_com.h.

Referenced by copy_dir(), and ushell_cmd_sync().

#define FS_DATE_CREATION TRUE

Definition at line 106 of file fs_com.h.

#define FS_DATE_LAST_WRITE FALSE

Definition at line 107 of file fs_com.h.

Referenced by fat_get_date().

#define FS_FILE TRUE

Definition at line 112 of file fs_com.h.

Referenced by fat_entry_check(), nav_dir_name(), nav_filelist_nb(), and nav_filelist_set().

#define FS_DIR FALSE

Definition at line 113 of file fs_com.h.

Referenced by fat_clear_entry_info_and_ptr(), fat_entry_check(), nav_dir_gotoparent(), nav_filelist_eol(), and nav_filelist_set().

#define FS_ID_DIR_EMPTY 0xFFFFFFFF

Definition at line 118 of file fs_com.h.

#define FS_ID_DIR_ROOT 0

Definition at line 119 of file fs_com.h.

#define FS_ATTR_FILE ((Byte)0x00)

Definition at line 124 of file fs_com.h.

#define FS_ATTR_READ_ONLY ((Byte)0x01)

Definition at line 125 of file fs_com.h.

Referenced by file_open(), and nav_file_isreadonly().

#define FS_ATTR_HIDDEN ((Byte)0x02)

Definition at line 126 of file fs_com.h.

#define FS_ATTR_SYSTEM ((Byte)0x04)

Definition at line 127 of file fs_com.h.

#define FS_ATTR_VOLUME_ID ((Byte)0x08)

Definition at line 128 of file fs_com.h.

Referenced by fat_entry_check().

#define FS_ATTR_DIRECTORY ((Byte)0x10)

Definition at line 129 of file fs_com.h.

Referenced by fat_entry_check(), and fat_entry_is_dir().

#define FS_ATTR_ARCHIVE ((Byte)0x20)

Definition at line 130 of file fs_com.h.

#define FS_ATTR_LFN_ENTRY ((Byte)0x0F)

Definition at line 131 of file fs_com.h.

Referenced by fat_entry_longname().

#define Fat_is_not_a_file ((FS_ATTR_DIRECTORY & fs_g_nav_entry.u8_attr) || (FS_ATTR_VOLUME_ID & fs_g_nav_entry.u8_attr))

Definition at line 132 of file fs_com.h.

Referenced by fat_check_is_file().

#define FOPEN_READ_ACCESS 0x01

Definition at line 137 of file fs_com.h.

Referenced by file_getc(), file_read(), and file_read_buf().

#define FOPEN_WRITE_ACCESS 0x02

Definition at line 138 of file fs_com.h.

Referenced by file_close(), and file_open().

#define FOPEN_CLEAR_SIZE 0x04

Definition at line 139 of file fs_com.h.

Referenced by file_open().

#define FOPEN_CLEAR_PTR 0x08

Definition at line 140 of file fs_com.h.

Referenced by file_open().

#define FOPEN_MODE_R (FOPEN_READ_ACCESS|FOPEN_CLEAR_PTR)

R access, flux pointer = 0, size not modify.

Definition at line 141 of file fs_com.h.

Referenced by firm_upgrade_run(), and ushell_cmd_cat().

#define FOPEN_MODE_R_PLUS (FOPEN_READ_ACCESS|FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR)

R/W access, flux pointer = 0, size not modify.

Definition at line 142 of file fs_com.h.

#define FOPEN_MODE_W (FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR|FOPEN_CLEAR_SIZE)

W access, flux pointer = 0, size = 0.

Definition at line 143 of file fs_com.h.

Referenced by firm_upgrade_status(), and ushell_cmd_perform_alloc().

#define FOPEN_MODE_W_PLUS (FOPEN_READ_ACCESS|FOPEN_WRITE_ACCESS|FOPEN_CLEAR_PTR|FOPEN_CLEAR_SIZE)

R/W access, flux pointer = 0, size = 0.

Definition at line 144 of file fs_com.h.

#define FOPEN_MODE_APPEND (FOPEN_WRITE_ACCESS)

W access, flux pointer = at the end, size not modify.

Definition at line 145 of file fs_com.h.

Referenced by ushell_cmd_append_file().

#define FS_EOF 0xFFFF

Definition at line 149 of file fs_com.h.

Referenced by file_getc().

#define FS_FORMAT_DEFAULT 0x01

The format routine chooses the better FAT for the device.

Definition at line 153 of file fs_com.h.

Referenced by ushell_cmd_format().

#define FS_FORMAT_FAT 0x02

Force FAT12 or FAT16 format.

Definition at line 154 of file fs_com.h.

#define FS_FORMAT_FAT32 0x03

Force FAT32 format.

Definition at line 155 of file fs_com.h.

#define FS_FORMAT_NOMBR_FLAG 0x80

MBR is mandatory for USB device on MacOS, and no MBR is mandatory for CD-ROM USB device on Windows.

Definition at line 156 of file fs_com.h.

#define FS_FORMAT_DEFAULT_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_DEFAULT)

Definition at line 157 of file fs_com.h.

#define FS_FORMAT_FAT_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_FAT)

Definition at line 158 of file fs_com.h.

#define FS_FORMAT_FAT32_NOMBR (FS_FORMAT_NOMBR_FLAG | FS_FORMAT_FAT32)

Definition at line 159 of file fs_com.h.

#define FS_ERR_HW (FAIL+0)

Hardware driver error.

Definition at line 187 of file fs_com.h.

Referenced by fat_cache_flush(), fat_cache_read_sector(), fat_check_device(), and file_read_buf().

#define FS_ERR_NO_FORMAT (FAIL+1)

The selected drive isn't formated.

Definition at line 188 of file fs_com.h.

Referenced by fat_mount().

#define FS_ERR_NO_PART (FAIL+2)

The selected partition doesn't existed.

Definition at line 189 of file fs_com.h.

Referenced by fat_mount().

#define FS_ERR_NO_SUPPORT_PART (FAIL+3)

The selected partition isn't supported.

Definition at line 190 of file fs_com.h.

Referenced by fat_mount().

#define FS_ERR_TOO_FILE_OPEN (FAIL+4)

The navigation have already opened a file.

Definition at line 191 of file fs_com.h.

Referenced by fat_check_noopen().

#define FS_ERR_END_OF_DRIVE (FAIL+5)

There are not other driver.

Definition at line 192 of file fs_com.h.

Referenced by nav_drive_set().

#define FS_ERR_BAD_POS (FAIL+6)

The position is over the file.

Definition at line 193 of file fs_com.h.

Referenced by file_seek().

#define FS_ERR_FS (FAIL+7)

File system error.

Definition at line 194 of file fs_com.h.

Referenced by fat_cluster_list(), nav_dir_gotoparent(), and nav_filelist_set().

#define FS_ERR_NO_FIND (FAIL+8)

File no found.

Definition at line 195 of file fs_com.h.

Referenced by nav_filelist_first(), nav_filelist_last(), and nav_filelist_set().

#define FS_ERR_ENTRY_EMPTY (FAIL+9)

File entry empty.

Definition at line 196 of file fs_com.h.

Referenced by fat_entry_check(), nav_filelist_set(), and nav_partition_label().

#define FS_ERR_ENTRY_BAD (FAIL+10)

File entry bad.

Definition at line 197 of file fs_com.h.

Referenced by fat_entry_check(), fat_entry_longname(), and nav_file_name().

#define FS_ERR_ENTRY_BADTYPE (FAIL+11)

File entry type don't corresponding.

Definition at line 198 of file fs_com.h.

#define FS_ERR_NO_DIR (FAIL+12)

The selected file isn't a directory.

Definition at line 199 of file fs_com.h.

Referenced by copy_dir(), fat_entry_is_dir(), and ushell_cmd_sync().

#define FS_ERR_NO_MOUNT (FAIL+13)

The partition isn't mounted.

Definition at line 200 of file fs_com.h.

Referenced by fat_check_mount().

#define FS_ERR_NO_FILE_SEL (FAIL+14)

There are no selected file.

Definition at line 201 of file fs_com.h.

Referenced by fat_check_select().

#define FS_NO_LAST_LFN_ENTRY (FAIL+15)

The file entry isn't the last long file entry.

Definition at line 202 of file fs_com.h.

Referenced by fat_entry_longname(), and nav_file_name().

#define FS_ERR_ID_FILE (FAIL+17)

The file identifier is bad.

Definition at line 204 of file fs_com.h.

#define FS_ERR_NO_FILE (FAIL+18)

The selected file entry isn't a file.

Definition at line 205 of file fs_com.h.

Referenced by fat_check_is_file().

#define FS_LUN_WP (FAIL+19)

Drive is in read only mode.

Definition at line 206 of file fs_com.h.

Referenced by fat_cache_flush(), and file_open().

#define FS_ERR_READ_ONLY (FAIL+20)

File is on read access only.

Definition at line 207 of file fs_com.h.

Referenced by file_open().

#define FS_ERR_NAME_INCORRECT (FAIL+21)

The name don't corresponding at the filter name.

Definition at line 208 of file fs_com.h.

Referenced by fat_entry_longname(), and fat_entry_shortname().

#define FS_ERR_FILE_NO_OPEN (FAIL+22)

No file is opened.

Definition at line 209 of file fs_com.h.

Referenced by fat_check_open().

#define FS_ERR_HW_NO_PRESENT (FAIL+23)

Device is not present.

Definition at line 210 of file fs_com.h.

Referenced by fat_check_device().

#define FS_ERR_IS_ROOT (FAIL+24)

There aren't parent because the current directory is a root directory.

Definition at line 211 of file fs_com.h.

Referenced by nav_dir_gotoparent(), and nav_getcwd().

#define FS_ERR_OUT_LIST (FAIL+25)

The position is outside the cluster list.

Definition at line 212 of file fs_com.h.

Referenced by fat_cluster_list(), fat_read_file(), file_getc(), file_read(), file_read_buf(), and nav_filelist_set().

#define FS_ERR_NO_FREE_SPACE (FAIL+26)

No free cluster found in FAT.

Definition at line 213 of file fs_com.h.

#define FS_ERR_INCORRECT_NAME (FAIL+27)

Incorrect name, this one cannot contain any of the following characters \/:*?"<>|.

Definition at line 214 of file fs_com.h.

#define FS_ERR_DIR_NOT_EMPTY (FAIL+28)

This function erases only file and empty directory.

Definition at line 215 of file fs_com.h.

#define FS_ERR_WRITE_ONLY (FAIL+29)

File is on write access only.

Definition at line 216 of file fs_com.h.

Referenced by file_getc(), file_read(), and file_read_buf().

#define FS_ERR_MODE_NOAVIALABLE (FAIL+30)

This open mode isn't available.

Definition at line 217 of file fs_com.h.

Referenced by file_open().

#define FS_ERR_EOF (FAIL+31)

End of file.

Definition at line 218 of file fs_com.h.

Referenced by file_getc(), file_read(), and file_read_buf().

#define FS_ERR_BAD_SIZE_FAT (FAIL+32)

The disk size is not supported by selected FAT format.

Definition at line 219 of file fs_com.h.

#define FS_ERR_COMMAND (FAIL+33)

This command is not supported.

Definition at line 220 of file fs_com.h.

Referenced by fat_cluster_val().

#define FS_ERR_BUFFER_FULL (FAIL+34)

Buffer is too small.

Definition at line 221 of file fs_com.h.

Referenced by nav_getcwd().

#define FS_ERR_COPY_DIR (FAIL+35)

Directory copy is not supported.

Definition at line 222 of file fs_com.h.

#define FS_ERR_COPY_RUNNING (FAIL+36)

A copy action is always running.

Definition at line 223 of file fs_com.h.

#define FS_ERR_COPY_IMPOSSIBLE (FAIL+37)

The copy is impossible.

Definition at line 224 of file fs_com.h.

#define FS_ERR_BAD_NAV (FAIL+38)

The navigator identifier doesn't existed.

Definition at line 225 of file fs_com.h.

Referenced by nav_select().

#define FS_ERR_FILE_OPEN (FAIL+39)

The file is already opened.

Definition at line 226 of file fs_com.h.

#define FS_ERR_FILE_OPEN_WR (FAIL+40)

The file is already opened in write mode.

Definition at line 227 of file fs_com.h.

#define FS_ERR_FILE_EXIST (FAIL+41)

The file is already existed.

Definition at line 228 of file fs_com.h.

Referenced by copy_dir(), firm_upgrade_status(), ushell_cmd_perform_alloc(), and ushell_cmd_sync().

#define FS_ERR_NAME_TOO_LARGE (FAIL+42)

The file name is too large (>260 characters).

Definition at line 229 of file fs_com.h.

#define FS_ERR_PL_NOT_OPEN (FAIL+50)

The play list isn't opened.

Definition at line 231 of file fs_com.h.

#define FS_ERR_PL_ALREADY_OPEN (FAIL+51)

The play list is already opened.

Definition at line 232 of file fs_com.h.

#define FS_ERR_PL_LST_END (FAIL+52)

You are at the end of play list.

Definition at line 233 of file fs_com.h.

#define FS_ERR_PL_LST_BEG (FAIL+53)

You are at the beginning of play list.

Definition at line 234 of file fs_com.h.

#define FS_ERR_PL_OUT_LST (FAIL+54)

You are outside of the play list.

Definition at line 235 of file fs_com.h.

#define FS_ERR_PL_READ_ONLY (FAIL+55)

Impossible to modify the play list.

Definition at line 236 of file fs_com.h.

#define FSFEATURE_READ 0x00

All read functions.

Definition at line 242 of file fs_com.h.

#define FSFEATURE_WRITE 0x02

nav_file_copy(), nav_file_paste(), nav_file_del(), file_create(), file_open(MODE_WRITE), file_write(), file_putc()

Definition at line 243 of file fs_com.h.

#define FSFEATURE_WRITE_COMPLET 0x06

FSFEATURE_WRITE + nav_drive_format(), nav_dir_make(), nav_file_rename(), nav_file_dateset(), nav_file_attributset().

Definition at line 244 of file fs_com.h.

#define FSFEATURE_ALL 0xFF

All file system module.

Definition at line 245 of file fs_com.h.

## Typedef Documentation

typedef U16 UNICODE

Definition at line 167 of file fs_com.h.

typedef char _MEM_TYPE_SLOW_* FS_STRING

Definition at line 168 of file fs_com.h.

typedef UNICODE _MEM_TYPE_SLOW_* FS_STR_UNICODE

Definition at line 169 of file fs_com.h.

typedef U8 Fs_status

Definition at line 250 of file fs_com.h.

## Variable Documentation

_MEM_TYPE_SLOW_ Fs_status fs_g_status

Referenced by copy_dir(), fat_cache_flush(), fat_cache_read_sector(), fat_check_device(), fat_check_is_file(), fat_check_mount(), fat_check_noopen(), fat_check_open(), fat_check_select(), fat_cluster_list(), fat_cluster_val(), fat_entry_check(), fat_entry_is_dir(), fat_entry_longname(), fat_entry_shortname(), fat_mount(), fat_read_file(), file_getc(), file_open(), file_read(), file_read_buf(), file_seek(), firm_upgrade_status(), nav_dir_gotoparent(), nav_drive_set(), nav_file_name(), nav_filelist_first(), nav_filelist_last(), nav_filelist_set(), nav_getcwd(), nav_partition_label(), nav_select(), ushell_cmd_perform_alloc(), and ushell_cmd_sync().