# scif_dfll_closedloop_conf_t Struct Reference

DFLL closed-loop mode settings. More...

`#include <scif_uc3l.h>`

## Data Fields
unsigned int | coarse
| The coarse value (= (fDFLL - SCIF_DFLL_MINFREQ_KHZ)*255/(SCIF_DFLL_MAXFREQ_KHZ - SCIF_DFLL_MINFREQ_KHZ)).
unsigned int | fmul
| The fmul value (= (fDFLL*2^16)/fref).
unsigned int | maxstep
| Maximum step size during coarse adjustment.

## Detailed Description

DFLL closed-loop mode settings.

Definition at line 203 of file scif_uc3l.h.

## Field Documentation

unsigned int scif_dfll_closedloop_conf_t::coarse

The coarse value (= (fDFLL - SCIF_DFLL_MINFREQ_KHZ)*255/(SCIF_DFLL_MAXFREQ_KHZ - SCIF_DFLL_MINFREQ_KHZ)).

Definition at line 206 of file scif_uc3l.h.

Referenced by local_start_dfll_clock(), scif_dfll0_closedloop_configure_and_start(), and scif_dfll0_closedloop_start().

unsigned int scif_dfll_closedloop_conf_t::fmul

The fmul value (= (fDFLL*2^16)/fref).

Definition at line 208 of file scif_uc3l.h.

Referenced by local_start_dfll_clock(), scif_dfll0_closedloop_configure_and_start(), and scif_dfll0_closedloop_start().

unsigned int scif_dfll_closedloop_conf_t::maxstep

Maximum step size during coarse adjustment.

Definition at line 210 of file scif_uc3l.h.

Referenced by local_start_dfll_clock(), scif_dfll0_closedloop_configure_and_start(), and scif_dfll0_closedloop_start().